|  |  |
| --- | --- |
| **DCS Network Repeaters/Nodes** | **G2/D-Plus Repeaters/Nodes** |
| <http://xreflector.net/neu3/>  All reflectors are available from one page. | <http://ref028.dstargateway.org>  Change the ref028 to which ever reflector you want. |
| Have access to REF and DCS reflectors. | Only have access to REF reflectors. |
| Has up to 26 “groups” for each reflector : A  Z | Has up to 4 “modules” - A  D |
| A worldwide “group” - A - where all “A groups” are linked together to provide a worldwide network. | Does not have a worldwide possibility but repeaters/nodes need to be connected to where you want to be heard. |
| The provision of “chat groups” on each reflector where repeaters and nodes can be connected for conversations in an ad-hoc manner so not as to tie up the main reflector. | No provision of chat groups and people need to call sign route but this is limited to 2 people or repeaters. |
| Provision of regional “groups” within a country. For example on DCS011 there is “worldwide”, “Belgium General”, “Flemish”, “French”, “Emergency” etc. | Some reflectors represent areas but the number is limited. |
| Repeaters have the ability to call sign and repeater route. | Repeaters have the ability to call sign and repeater route. |
| Last Heard list available. | Last Heard list available. |
| Not easy to locate the last place someone transmitted if this was through a node.  However, the same functionality as G2/D-Plus is available through a repeater on [www.jfindu.net](http://www.jfindu.net) | Easy to identify where a person last transmitted with [www.jfindu.net](http://www.jfindu.net) |